Skip to content

#
GustavoIFelippe / Templates-Zabbix-Fiberhome Public

- Notifications
- Star 4
- Fork 3

Permalink
main
Switch branches/tags

## Templates-Zabbix-Fiberhome/GEPON-OLT-COMMON-MIB.txt

Go to file
GustavoIFelippe Add files via upload
Latest commit 717266a May 24, 2021
History
1 contributor

### Users who have contributed to this file

7043 lines (5834 sloc) 159 KB
Raw Blame

| --
| -- GEPON-OLT-COMMON-MIB.my
| -- MIB generated by MG-SOFT Visual MIB Builder Version 5.0 Build 250
| -- Wednesday, June 08, 2011 at 11:42:11
| --
| -- GEPON-OLT-COMMON-MIB.my
| -- MIB generated by MG-SOFT Visual MIB Builder Version 5.0 Build 250
| -- Tuesday, June 07, 2011 at 16:34:40
| --
| -- File Name : GEPON-OLT-COMMON-MIB.mib
| -- Date : Fri May 13 09:50:16 CST 2011
| -- Author : AdventNet Agent Toolkit C Edition - MibEditor 6
| --
| -- GEPON-OLT-COMMON-MIB.mib
| -- MIB generated by MG-SOFT Visual MIB Builder Version 5.0 Build 250
| -- Thursday, September 30, 2010 at 11:12:51
| --
| -- GEPON-OLT-COMMON-MIB.mib
| -- MIB generated by MG-SOFT Visual MIB Builder Version 5.0 Build 250
| -- Tuesday, September 28, 2010 at 14:05:57
| --
| -- File Name : GEPON-OLT-COMMON-MIB.mib
| -- Date : Fri Sep 17 15:29:45 CST 2010
| -- Author : AdventNet Agent Toolkit C Edition - MibEditor 6
| -- V2.001 replace stream by traffic,add some nodes to dslPerformance and so on CWT 20100118
| -- V2.002 add available number OID and available list OID for adsl pvc vlan CWT 20100122
| -- V2.003 imports dsl performance from rfc2662 CWT 20100126
| -- v2.004 dslam performance self-definition,yangdan,20100210
| -- v2.005 add ftthLogicWhiteListTable and divide portEnable to two table CWT 20100308
| GEPON-OLT-COMMON-MIB DEFINITIONS ::= BEGIN
| IMPORTS
| ifIndex
| FROM IF-MIB
| enterprises, IpAddress, Integer32, Unsigned32, OBJECT-TYPE
| FROM SNMPv2-SMI
| MacAddress, RowStatus, TruthValue, TEXTUAL-CONVENTION, DateAndTime
| FROM SNMPv2-TC;
| --
| -- Textual conventions
| --
| -- Textual conventions
| --
| -- TEXTUAL-CONVENTIONS --
| MyTC ::= TEXTUAL-CONVENTION
| STATUS current
| DESCRIPTION
| "TC Description"
| SYNTAX Integer32
| --
| -- Node definitions
| --
| -- Node definitions
| --
| -- 1.3.6.1.4.1.5875
| -- 1.3.6.1.4.1.5875
| fiberhome OBJECT IDENTIFIER ::= { enterprises 5875 }
| -- 1.3.6.1.4.1.5875.800
| -- 1.3.6.1.4.1.5875.800
| standard OBJECT IDENTIFIER ::= { fiberhome 800 }
| -- 1.3.6.1.4.1.5875.800.3
| -- 1.3.6.1.4.1.5875.800.3
| oltData OBJECT IDENTIFIER ::= { standard 3 }
| -- 1.3.6.1.4.1.5875.800.3.1
| -- 1.3.6.1.4.1.5875.800.3.1
| onuWhiteList OBJECT IDENTIFIER ::= { oltData 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.1
| onuPhysicalwhiteListTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuPhysicalwhiteListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuWhiteList 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.1.1
| onuPhysicalwhiteListEntry OBJECT-TYPE
| SYNTAX OnuPhysicalwhiteListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuAuthNo1 }
| ::= { onuPhysicalwhiteListTable 1 }
| OnuPhysicalwhiteListEntry ::=
| SEQUENCE {
| onuAuthNo1
| Unsigned32,
| onuSlotForPhysical
| Integer32,
| onuPonForPhysical
| Integer32,
| onuMacForPhysical
| OCTET STRING,
| actionForPhysical
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.1
| onuAuthNo1 OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicalwhiteListEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.2
| onuSlotForPhysical OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicalwhiteListEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.3
| onuPonForPhysical OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicalwhiteListEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.4
| onuMacForPhysical OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicalwhiteListEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.1.1.1.5
| actionForPhysical OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "4-create
| 6-destroy"
| ::= { onuPhysicalwhiteListEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.1.2
| -- 1.3.6.1.4.1.5875.800.3.1.2
| onuLogicWhiteListTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuLogicWhiteListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuWhiteList 2 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1
| -- 1.3.6.1.4.1.5875.800.3.1.2.1
| onuLogicWhiteListEntry OBJECT-TYPE
| SYNTAX OnuLogicWhiteListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuAuthNo2 }
| ::= { onuLogicWhiteListTable 1 }
| OnuLogicWhiteListEntry ::=
| SEQUENCE {
| onuAuthNo2
| Unsigned32,
| onuSlotForLogic
| Integer32,
| onuPonForLogic
| Integer32,
| onuSnForLogic
| OCTET STRING,
| onuSnPasswordForLogic
| OCTET STRING,
| actionForLogic
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.1
| onuAuthNo2 OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuLogicWhiteListEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.2
| onuSlotForLogic OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuLogicWhiteListEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.3
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.3
| onuPonForLogic OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuLogicWhiteListEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.4
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.4
| onuSnForLogic OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuLogicWhiteListEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.5
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.5
| onuSnPasswordForLogic OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuLogicWhiteListEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.6
| -- 1.3.6.1.4.1.5875.800.3.1.2.1.6
| actionForLogic OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "4-create
| 6-destroy"
| ::= { onuLogicWhiteListEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.1.3
| -- 1.3.6.1.4.1.5875.800.3.1.3
| applyCommand OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "apply sn-whitelist or mac-whitelist to service card"
| ::= { onuWhiteList 3 }
| -- 1.3.6.1.4.1.5875.800.3.1.4
| -- 1.3.6.1.4.1.5875.800.3.1.4
| onuMacListFor5516Table OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuMacListFor5516Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuWhiteList 4 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1
| -- 1.3.6.1.4.1.5875.800.3.1.4.1
| onuMacListFor5516Entry OBJECT-TYPE
| SYNTAX OnuMacListFor5516Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { macListId }
| ::= { onuMacListFor5516Table 1 }
| OnuMacListFor5516Entry ::=
| SEQUENCE {
| macListId
| Integer32,
| slotNoForMacList
| Integer32,
| ponNoForMacList
| Integer32,
| onuNoForMacList
| Integer32,
| onuTypeForMacList
| Integer32,
| macForMacList
| MacAddress,
| passwordForMacList
| OCTET STRING,
| actionForMacList
| RowStatus
| }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.1
| macListId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.2
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.2
| slotNoForMacList OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 2 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.3
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.3
| ponNoForMacList OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 3 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.4
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.4
| onuNoForMacList OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 4 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.5
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.5
| onuTypeForMacList OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 5 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.6
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.6
| macForMacList OBJECT-TYPE
| SYNTAX MacAddress (SIZE (6))
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 6 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.7
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.7
| passwordForMacList OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 7 }
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.8
| -- 1.3.6.1.4.1.5875.800.3.1.4.1.8
| actionForMacList OBJECT-TYPE
| SYNTAX RowStatus
| {
| active(1),
| notInService(2),
| notReady(3),
| createAndGo(4),
| createAndWait(5),
| destroy(6)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuMacListFor5516Entry 8 }
| -- 1.3.6.1.4.1.5875.800.3.1.5
| -- 1.3.6.1.4.1.5875.800.3.1.5
| onuSnListFor5516Table OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuSnListFor5516Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuWhiteList 5 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1
| -- 1.3.6.1.4.1.5875.800.3.1.5.1
| onuSnListFor5516Entry OBJECT-TYPE
| SYNTAX OnuSnListFor5516Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { snListId }
| ::= { onuSnListFor5516Table 1 }
| OnuSnListFor5516Entry ::=
| SEQUENCE {
| snListId
| Integer32,
| slotNoForSnList
| Integer32,
| ponNoForSnList
| Integer32,
| onuNoForSnList
| Integer32,
| onuTypeForSnList
| Integer32,
| snForSnList
| OCTET STRING,
| passwordForSnList
| OCTET STRING,
| actionForSnList
| RowStatus
| }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.1
| snListId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 1 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.2
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.2
| slotNoForSnList OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 2 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.3
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.3
| ponNoForSnList OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 3 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.4
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.4
| onuNoForSnList OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 4 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.5
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.5
| onuTypeForSnList OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 5 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.6
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.6
| snForSnList OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 6 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.7
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.7
| passwordForSnList OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 7 }
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.8
| -- 1.3.6.1.4.1.5875.800.3.1.5.1.8
| actionForSnList OBJECT-TYPE
| SYNTAX RowStatus
| {
| active(1),
| notInService(2),
| notReady(3),
| createAndGo(4),
| createAndWait(5),
| destroy(6)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnListFor5516Entry 8 }
| -- 1.3.6.1.4.1.5875.800.3.2
| -- 1.3.6.1.4.1.5875.800.3.2
| interfaceEnable OBJECT IDENTIFIER ::= { oltData 2 }
| -- 1.3.6.1.4.1.5875.800.3.2.1
| -- 1.3.6.1.4.1.5875.800.3.2.1
| voicePortEnableTable OBJECT-TYPE
| SYNTAX SEQUENCE OF VoicePortEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceEnable 1 }
| -- 1.3.6.1.4.1.5875.800.3.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.2.1.1
| voicePortEnableEntry OBJECT-TYPE
| SYNTAX VoicePortEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { potsIndex }
| ::= { voicePortEnableTable 1 }
| VoicePortEnableEntry ::=
| SEQUENCE {
| potsPortEnable
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.2.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.2.1.1.2
| potsPortEnable OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "0-disable
| 1-enable"
| ::= { voicePortEnableEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.2.2
| -- 1.3.6.1.4.1.5875.800.3.2.2
| dataPortEnableTable OBJECT-TYPE
| SYNTAX SEQUENCE OF DataPortEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceEnable 2 }
| -- 1.3.6.1.4.1.5875.800.3.2.2.1
| -- 1.3.6.1.4.1.5875.800.3.2.2.1
| dataPortEnableEntry OBJECT-TYPE
| SYNTAX DataPortEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { dataPortEnableTable 1 }
| DataPortEnableEntry ::=
| SEQUENCE {
| dataPortEnable
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.2.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.2.2.1.2
| dataPortEnable OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "0-disable
| 1-enable"
| ::= { dataPortEnableEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.2.3
| -- 1.3.6.1.4.1.5875.800.3.2.3
| oltPonEnableTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OltPonEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceEnable 3 }
| -- 1.3.6.1.4.1.5875.800.3.2.3.1
| -- 1.3.6.1.4.1.5875.800.3.2.3.1
| oltPonEnableEntry OBJECT-TYPE
| SYNTAX OltPonEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { ponIndex }
| ::= { oltPonEnableTable 1 }
| OltPonEnableEntry ::=
| SEQUENCE {
| oltPonEnable
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.2.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.2.3.1.1
| oltPonEnable OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:enable
| 0:disable"
| ::= { oltPonEnableEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.3
| -- 1.3.6.1.4.1.5875.800.3.3
| onuPortConfig OBJECT IDENTIFIER ::= { oltData 3 }
| -- 1.3.6.1.4.1.5875.800.3.3.1
| -- 1.3.6.1.4.1.5875.800.3.3.1
| bandwidthProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF BandwidthProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPortConfig 1 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.3.1.1
| bandwidthProfileEntry OBJECT-TYPE
| SYNTAX BandwidthProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { bandwidthProfileId }
| ::= { bandwidthProfileTable 1 }
| BandwidthProfileEntry ::=
| SEQUENCE {
| bandwidthProfileId
| Integer32,
| bandwidthProfileName
| OCTET STRING,
| upMinRate
| Integer32,
| upMaxRate
| Integer32,
| downMinRate
| Integer32,
| downMaxRate
| Integer32,
| fixedRate
| Integer32,
| bandwidthProfileAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.1
| bandwidthProfileId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.2
| bandwidthProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.3
| upMinRate OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.4
| upMaxRate OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.5
| downMinRate OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.6
| downMaxRate OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.7
| fixedRate OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { bandwidthProfileEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.12
| -- 1.3.6.1.4.1.5875.800.3.3.1.1.12
| bandwidthProfileAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "1-active
| 4-create
| 6-destroy
| 7-modify"
| ::= { bandwidthProfileEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.3.2
| -- 1.3.6.1.4.1.5875.800.3.3.2
| attachPortBandwidthProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF AttachPortBandwidthProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPortConfig 2 }
| -- 1.3.6.1.4.1.5875.800.3.3.2.1
| -- 1.3.6.1.4.1.5875.800.3.3.2.1
| attachPortBandwidthProfileEntry OBJECT-TYPE
| SYNTAX AttachPortBandwidthProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { fttbIfIndex }
| ::= { attachPortBandwidthProfileTable 1 }
| AttachPortBandwidthProfileEntry ::=
| SEQUENCE {
| fttbIfIndex
| Unsigned32,
| attachBandwidthProfileId
| Integer32,
| attachBandwidthProfileName
| OCTET STRING,
| setDefaultBandwidthProfileAction
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.1
| fttbIfIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { attachPortBandwidthProfileEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.2
| attachBandwidthProfileId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachPortBandwidthProfileEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.4
| -- 1.3.6.1.4.1.5875.800.3.3.2.1.4
| attachBandwidthProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { attachPortBandwidthProfileEntry 4 }
| setDefaultBandwidthProfileAction OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 1 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { attachPortBandwidthProfileEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.3.3
| -- 1.3.6.1.4.1.5875.800.3.3.3
| portAttributeProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PortAttributeProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPortConfig 3 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1
| -- 1.3.6.1.4.1.5875.800.3.3.3.1
| portAttributeProfileEntry OBJECT-TYPE
| SYNTAX PortAttributeProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portAttributeProfileId }
| ::= { portAttributeProfileTable 1 }
| PortAttributeProfileEntry ::=
| SEQUENCE {
| portAttributeProfileId
| Integer32,
| portAttributeProfileName
| OCTET STRING,
| autoNegotiation
| INTEGER,
| speed
| Integer32,
| duplex
| INTEGER,
| flowControl
| INTEGER,
| portAttributeProfileAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.1
| portAttributeProfileId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { portAttributeProfileEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.2
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.2
| portAttributeProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { portAttributeProfileEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.3
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.3
| autoNegotiation OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0),
| disableFor5116(2)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 5516:
| 1:enable
| 0:disable
| 5116:
| 1:enable
| 2:disableFor5116
| "
| ::= { portAttributeProfileEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.4
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.4
| speed OBJECT-TYPE
| SYNTAX Integer32 (0..2)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 0:10M
| 1:100M
| 2:1000M"
| ::= { portAttributeProfileEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.5
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.5
| duplex OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:enable
| 0:disable"
| ::= { portAttributeProfileEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.6
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.6
| flowControl OBJECT-TYPE
| SYNTAX INTEGER
| {
| enable(1),
| disable(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:enable
| 0:disable"
| ::= { portAttributeProfileEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.10
| -- 1.3.6.1.4.1.5875.800.3.3.3.1.10
| portAttributeProfileAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description
| 4:create
| 6:destroy
| 7:modify"
| ::= { portAttributeProfileEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.3.4
| -- 1.3.6.1.4.1.5875.800.3.3.4
| attachPortAttributeProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF AttachPortAttributeProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPortConfig 4 }
| -- 1.3.6.1.4.1.5875.800.3.3.4.1
| -- 1.3.6.1.4.1.5875.800.3.3.4.1
| attachPortAttributeProfileEntry OBJECT-TYPE
| SYNTAX AttachPortAttributeProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { attachPortAttributeProfileTable 1 }
| AttachPortAttributeProfileEntry ::=
| SEQUENCE {
| attachPortAttributeProfileName
| OCTET STRING,
| setDefaultPortAttributeProfileAction
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.3.4.1.1
| -- 1.3.6.1.4.1.5875.800.3.3.4.1.1
| attachPortAttributeProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachPortAttributeProfileEntry 1 }
| setDefaultPortAttributeProfileAction OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 1 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { attachPortAttributeProfileEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.3.10
| -- 1.3.6.1.4.1.5875.800.3.3.10
| getNextPortProfileId OBJECT IDENTIFIER ::= { onuPortConfig 10 }
| -- 1.3.6.1.4.1.5875.800.3.3.10.1
| -- 1.3.6.1.4.1.5875.800.3.3.10.1
| getNextBandwidthProfileId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { getNextPortProfileId 1 }
| -- 1.3.6.1.4.1.5875.800.3.3.10.2
| -- 1.3.6.1.4.1.5875.800.3.3.10.2
| getNextPortAttributeProfileId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { getNextPortProfileId 2 }
| -- 1.3.6.1.4.1.5875.800.3.5
| -- 1.3.6.1.4.1.5875.800.3.5
| feServiceConfigure OBJECT IDENTIFIER ::= { oltData 5 }
| -- 1.3.6.1.4.1.5875.800.3.5.1
| -- 1.3.6.1.4.1.5875.800.3.5.1
| feServiceCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FeServiceCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { feServiceConfigure 1 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.5.1.1
| feServiceCfgEntry OBJECT-TYPE
| SYNTAX FeServiceCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex, serviceId }
| ::= { feServiceCfgTable 1 }
| FeServiceCfgEntry ::=
| SEQUENCE {
| serviceId
| Integer32,
| serviceType
| Integer32,
| cvlanMode
| INTEGER,
| cvlan
| Integer32,
| cvlanCos
| Integer32,
| tvlan
| Integer32,
| tvlanCos
| Integer32,
| svlan
| Integer32,
| svlanCos
| Integer32,
| upMinBandWidth
| Integer32,
| upManBandWidth
| Integer32,
| dnBandWidth
| Integer32,
| serviceVlanName
| OCTET STRING,
| qinqProfileName
| OCTET STRING,
| feServiceCfgAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.1
| serviceId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { feServiceCfgEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.2
| serviceType OBJECT-TYPE
| SYNTAX Integer32 (0..1)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 0:unicast
| 1:mulitcast"
| ::= { feServiceCfgEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.3
| cvlanMode OBJECT-TYPE
| SYNTAX INTEGER { tag(1), transparent(3) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:tag
| 3:transparent"
| ::= { feServiceCfgEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.4
| cvlan OBJECT-TYPE
| SYNTAX Integer32 (1..4085)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1~4085"
| ::= { feServiceCfgEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.5
| cvlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 0~7"
| ::= { feServiceCfgEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.6
| tvlan OBJECT-TYPE
| SYNTAX Integer32 (1..4085 | 65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1.value:1~4085
| 2:65535 interpreter(off)"
| ::= { feServiceCfgEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.7
| tvlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7 | 255)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| value:0~7"
| ::= { feServiceCfgEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.8
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.8
| svlan OBJECT-TYPE
| SYNTAX Integer32 (1..4085 | 65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:value(1~4085)
| 2:65535(QINQ off)"
| ::= { feServiceCfgEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.9
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.9
| svlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7 | 255)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| value:0~7"
| ::= { feServiceCfgEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.10
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.10
| upMinBandWidth OBJECT-TYPE
| SYNTAX Integer32 (0..1000000)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| value:0~1000000"
| ::= { feServiceCfgEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.11
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.11
| upManBandWidth OBJECT-TYPE
| SYNTAX Integer32 (256..1000000)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| value:256~1000000"
| ::= { feServiceCfgEntry 11 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.12
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.12
| dnBandWidth OBJECT-TYPE
| SYNTAX Integer32 (0..1000000)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| value:0~1000000"
| ::= { feServiceCfgEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.15
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.15
| serviceVlanName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { feServiceCfgEntry 15 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.16
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.16
| qinqProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| if the qinq off, the value is meaningless"
| ::= { feServiceCfgEntry 16 }
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.20
| -- 1.3.6.1.4.1.5875.800.3.5.1.1.20
| feServiceCfgAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:create(4)
| 2:destroy(6)
| 3:modify(7)"
| ::= { feServiceCfgEntry 20 }
| -- 1.3.6.1.4.1.5875.800.3.5.2
| -- 1.3.6.1.4.1.5875.800.3.5.2
| feServiceCfgIdTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FeServiceCfgIdEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { feServiceConfigure 2 }
| -- 1.3.6.1.4.1.5875.800.3.5.2.1
| -- 1.3.6.1.4.1.5875.800.3.5.2.1
| feServiceCfgIdEntry OBJECT-TYPE
| SYNTAX FeServiceCfgIdEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { feServiceCfgIdTable 1 }
| FeServiceCfgIdEntry ::=
| SEQUENCE {
| nextServiceId
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.5.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.5.2.1.1
| nextServiceId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { feServiceCfgIdEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.5.3
| -- 1.3.6.1.4.1.5875.800.3.5.3
| feServiceCfgApplyTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FeServiceCfgApplyEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { feServiceConfigure 3 }
| -- 1.3.6.1.4.1.5875.800.3.5.3.1
| -- 1.3.6.1.4.1.5875.800.3.5.3.1
| feServiceCfgApplyEntry OBJECT-TYPE
| SYNTAX FeServiceCfgApplyEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { feServiceCfgApplyTable 1 }
| FeServiceCfgApplyEntry ::=
| SEQUENCE {
| feServiceCfgApplyCommand
| TruthValue
| }
| -- 1.3.6.1.4.1.5875.800.3.5.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.5.3.1.1
| feServiceCfgApplyCommand OBJECT-TYPE
| SYNTAX TruthValue
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { feServiceCfgApplyEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7
| -- 1.3.6.1.4.1.5875.800.3.7
| qinq OBJECT IDENTIFIER ::= { oltData 7 }
| -- 1.3.6.1.4.1.5875.800.3.7.2
| -- 1.3.6.1.4.1.5875.800.3.7.2
| attachQINQProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF AttachQINQProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 2 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1
| -- 1.3.6.1.4.1.5875.800.3.7.2.1
| attachQINQProfileEntry OBJECT-TYPE
| SYNTAX AttachQINQProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { attachQINQProfileName }
| ::= { attachQINQProfileTable 1 }
| AttachQINQProfileEntry ::=
| SEQUENCE {
| attachQINQProfileId
| Integer32,
| attachQINQProfileName
| OCTET STRING,
| attachQINQSvlan
| Integer32,
| attachQINQTpid
| Integer32,
| attachQINQCos
| Integer32,
| attachQINQProfileAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.1
| attachQINQProfileId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachQINQProfileEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.2
| attachQINQProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachQINQProfileEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.3
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.3
| attachQINQSvlan OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachQINQProfileEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.4
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.4
| attachQINQTpid OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachQINQProfileEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.5
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.5
| attachQINQCos OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attachQINQProfileEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.6
| -- 1.3.6.1.4.1.5875.800.3.7.2.1.6
| attachQINQProfileAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| create(4),
| destroy(6)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "4-create
| 6-delete
| 7-modify"
| ::= { attachQINQProfileEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.7.3
| -- 1.3.6.1.4.1.5875.800.3.7.3
| attchQinqProfileToOnuTable OBJECT-TYPE
| SYNTAX SEQUENCE OF AttchQinqProfileToOnuEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 3 }
| -- 1.3.6.1.4.1.5875.800.3.7.3.1
| -- 1.3.6.1.4.1.5875.800.3.7.3.1
| attchQinqProfileToOnuEntry OBJECT-TYPE
| SYNTAX AttchQinqProfileToOnuEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { attchQinqProfileToOnuTable 1 }
| AttchQinqProfileToOnuEntry ::=
| SEQUENCE {
| attchQinqProfileName
| OCTET STRING,
| qinqAttchAction
| Integer32,
| getOnuQinqProfileName
| OCTET STRING
| }
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.1
| attchQinqProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { attchQinqProfileToOnuEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.2
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.2
| qinqAttchAction OBJECT-TYPE
| SYNTAX Integer32 (0..1)
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Description:
| 1:bind(1)
| 2:unbind(0)"
| ::= { attchQinqProfileToOnuEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.3
| -- 1.3.6.1.4.1.5875.800.3.7.3.1.3
| getOnuQinqProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { attchQinqProfileToOnuEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.7.4
| -- 1.3.6.1.4.1.5875.800.3.7.4
| qinqBandWidthCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF QinqBandWidthCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 4 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1
| -- 1.3.6.1.4.1.5875.800.3.7.4.1
| qinqBandWidthCfgEntry OBJECT-TYPE
| SYNTAX QinqBandWidthCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex, onuQinqProfileName, qinqServiceId }
| ::= { qinqBandWidthCfgTable 1 }
| QinqBandWidthCfgEntry ::=
| SEQUENCE {
| onuQinqProfileName
| OCTET STRING,
| qinqServiceId
| Integer32,
| usMinBandwidth
| Integer32,
| usMaxBandwidth
| Integer32,
| usBurstBandwidth
| Integer32,
| dsMinBandwidth
| Integer32,
| dsMaxBandwidth
| Integer32,
| dsBurstBandwidth
| Integer32,
| qinqBandwidthCfgAction
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.1
| onuQinqProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.2
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.2
| qinqServiceId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.3
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.3
| usMinBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.4
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.4
| usMaxBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.5
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.5
| usBurstBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.6
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.6
| dsMinBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.7
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.7
| dsMaxBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.8
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.8
| dsBurstBandwidth OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.20
| -- 1.3.6.1.4.1.5875.800.3.7.4.1.20
| qinqBandwidthCfgAction OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandWidthCfgEntry 20 }
| -- 1.3.6.1.4.1.5875.800.3.7.5
| -- 1.3.6.1.4.1.5875.800.3.7.5
| qinqBandwidthCfgApplyTable OBJECT-TYPE
| SYNTAX SEQUENCE OF QinqBandwidthCfgApplyEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 5 }
| -- 1.3.6.1.4.1.5875.800.3.7.5.1
| -- 1.3.6.1.4.1.5875.800.3.7.5.1
| qinqBandwidthCfgApplyEntry OBJECT-TYPE
| SYNTAX QinqBandwidthCfgApplyEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { qinqBandwidthCfgApplyTable 1 }
| QinqBandwidthCfgApplyEntry ::=
| SEQUENCE {
| qinqBandwidthCfgApply
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.7.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.5.1.1
| qinqBandwidthCfgApply OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqBandwidthCfgApplyEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.7
| -- 1.3.6.1.4.1.5875.800.3.7.7
| qinqDomainTable OBJECT-TYPE
| SYNTAX SEQUENCE OF QinqDomainEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 7 }
| -- 1.3.6.1.4.1.5875.800.3.7.7.1
| -- 1.3.6.1.4.1.5875.800.3.7.7.1
| qinqDomainEntry OBJECT-TYPE
| SYNTAX QinqDomainEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { qinqDomainName }
| ::= { qinqDomainTable 1 }
| QinqDomainEntry ::=
| SEQUENCE {
| qinqDomainName
| OCTET STRING,
| qinqDomainAction
| RowStatus,
| qinqDomainServiceNum
| Integer32,
| nextQinqDomainServiceId
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.1
| qinqDomainName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqDomainEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.4
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.4
| qinqDomainAction OBJECT-TYPE
| SYNTAX RowStatus
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqDomainEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.5
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.5
| qinqDomainServiceNum OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqDomainEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.6
| -- 1.3.6.1.4.1.5875.800.3.7.7.1.6
| nextQinqDomainServiceId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqDomainEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.7.8
| -- 1.3.6.1.4.1.5875.800.3.7.8
| qinqDomainServiceTable OBJECT-TYPE
| SYNTAX SEQUENCE OF QinqDomainServiceEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinq 8 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1
| -- 1.3.6.1.4.1.5875.800.3.7.8.1
| qinqDomainServiceEntry OBJECT-TYPE
| SYNTAX QinqDomainServiceEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { qinqDomainName, qinqDomainServiceId }
| ::= { qinqDomainServiceTable 1 }
| QinqDomainServiceEntry ::=
| SEQUENCE {
| qinqDomainServiceId
| Integer32,
| qinqDomainServiceType
| INTEGER,
| qinqDomainLayer1OldVlan
| Integer32,
| qinqDomainLayer1OldVlanCos
| Integer32,
| qinqDomainLayer1VlanAction
| Integer32,
| qinqDomainLayer1VlanCos
| Integer32,
| qinqDomainLayer1Tpid
| Integer32,
| qinqDomainLayer1NewVlan
| Integer32,
| qinqDomainLayer2OldVlan
| Integer32,
| qinqDomainLayer2OldVlanCos
| Integer32,
| qinqDomainLayer2VlanAction
| Integer32,
| qinqDomainLayer2VlanCos
| Integer32,
| qinqDomainLayer2Tpid
| Integer32,
| qinqDomainLayer2NewVlan
| Integer32,
| qinqDomainUpRuleType
| Integer32,
| qinqDomainUpRuleValue
| OCTET STRING,
| qinqDomainUpRuleOperation
| Integer32,
| qinqDomainDnRuleType
| Integer32,
| qinqDomainDnRuleValue
| OCTET STRING,
| qinqDomainDnRuleOperation
| Integer32,
| getNextQinqDomainServiceRuleID
| Integer32,
| qinqDomainServiceAction
| RowStatus
| }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.1
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.1
| qinqDomainServiceId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { qinqDomainServiceEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.2
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.2
| qinqDomainServiceType OBJECT-TYPE
| SYNTAX INTEGER
| {
| single(0),
| shared(1)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description
| 0:Single
| 1:Shared"
| ::= { qinqDomainServiceEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.4
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.4
| qinqDomainLayer1OldVlan OBJECT-TYPE
| SYNTAX Integer32 (0..4085 | 65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| value:0~4085
| 0xffff(65535)"
| ::= { qinqDomainServiceEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.5
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.5
| qinqDomainLayer1OldVlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| value:0~7"
| ::= { qinqDomainServiceEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.6
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.6
| qinqDomainLayer1VlanAction OBJECT-TYPE
| SYNTAX Integer32 (0..3)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:add
| 2:interpret
| 3:transparent"
| ::= { qinqDomainServiceEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.7
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.7
| qinqDomainLayer1VlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7 | 255)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:value:0~7;
| 2:255(null)"
| ::= { qinqDomainServiceEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.8
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.8
| qinqDomainLayer1Tpid OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.9
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.9
| qinqDomainLayer1NewVlan OBJECT-TYPE
| SYNTAX Integer32 (1..4085 | 65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:value 1~4085
| 2: 0xffff(null)"
| ::= { qinqDomainServiceEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.10
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.10
| qinqDomainLayer2OldVlan OBJECT-TYPE
| SYNTAX Integer32 (0..65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:value 0~4085
| 2:0xffff"
| ::= { qinqDomainServiceEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.11
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.11
| qinqDomainLayer2OldVlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| value:0~7"
| ::= { qinqDomainServiceEntry 11 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.12
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.12
| qinqDomainLayer2VlanAction OBJECT-TYPE
| SYNTAX Integer32 (1..3)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:add
| 2:interpret
| 3:transparent"
| ::= { qinqDomainServiceEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.13
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.13
| qinqDomainLayer2VlanCos OBJECT-TYPE
| SYNTAX Integer32 (0..7 | 255)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:value 0~7
| 2:oxff(null)"
| ::= { qinqDomainServiceEntry 13 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.14
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.14
| qinqDomainLayer2Tpid OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 14 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.15
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.15
| qinqDomainLayer2NewVlan OBJECT-TYPE
| SYNTAX Integer32 (1..4085 | 65535)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:value0~4085
| 2:65535(null)"
| ::= { qinqDomainServiceEntry 15 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.30
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.30
| qinqDomainUpRuleType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 30 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.31
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.31
| qinqDomainUpRuleValue OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 31 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.32
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.32
| qinqDomainUpRuleOperation OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 32 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.33
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.33
| qinqDomainDnRuleType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 33 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.34
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.34
| qinqDomainDnRuleValue OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 34 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.35
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.35
| qinqDomainDnRuleOperation OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 35 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.36
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.36
| getNextQinqDomainServiceRuleID OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { qinqDomainServiceEntry 36 }
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.100
| -- 1.3.6.1.4.1.5875.800.3.7.8.1.100
| qinqDomainServiceAction OBJECT-TYPE
| SYNTAX RowStatus
| {
| active(1),
| notInService(2),
| notReady(3),
| createAndGo(4),
| createAndWait(5),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Description"
| ::= { qinqDomainServiceEntry 100 }
| qinqDomainServiceRuleTable OBJECT-TYPE
| SYNTAX SEQUENCE OF QinqDomainServiceRuleEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { qinq 9 }
| qinqDomainServiceRuleEntry OBJECT-TYPE
| SYNTAX QinqDomainServiceRuleEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { qinqDomainName, qinqDomainServiceId, qinqDomainServiceRuleIndex }
| ::= { qinqDomainServiceRuleTable 1 }
| QinqDomainServiceRuleEntry ::= SEQUENCE {
| qinqDomainServiceRuleIndex Integer32,
| qinqDomainServiceUpRuleType Integer32,
| qinqDomainServiceUpRuleValue OCTET STRING,
| qinqDomainServiceUpRuleOperation Integer32,
| qinqDomainServiceDnRuleType Integer32,
| qinqDomainServiceDnRuleValue OCTET STRING,
| qinqDomainServiceDnRuleOperation Integer32,
| qinqDomainServiceRuleAction RowStatus
| }
| qinqDomainServiceRuleIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 3 }
| qinqDomainServiceUpRuleType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 4 }
| qinqDomainServiceUpRuleValue OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 5 }
| qinqDomainServiceUpRuleOperation OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 6 }
| qinqDomainServiceDnRuleType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 7 }
| qinqDomainServiceDnRuleValue OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 8 }
| qinqDomainServiceDnRuleOperation OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 9 }
| qinqDomainServiceRuleAction OBJECT-TYPE
| SYNTAX RowStatus { active ( 1 ) , createAndGo ( 4 ) , destroy ( 6 ) , modify ( 7 ) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION "Column Description"
| ::= { qinqDomainServiceRuleEntry 20 }
| -- 1.3.6.1.4.1.5875.800.3.8
| -- 1.3.6.1.4.1.5875.800.3.8
| ftthPerformance OBJECT IDENTIFIER ::= { oltData 8 }
| -- 1.3.6.1.4.1.5875.800.3.8.1
| -- 1.3.6.1.4.1.5875.800.3.8.1
| ftthPerformanceCardEnableTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FtthPerformanceCardEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { ftthPerformance 1 }
| -- 1.3.6.1.4.1.5875.800.3.8.1.1
| -- 1.3.6.1.4.1.5875.800.3.8.1.1
| ftthPerformanceCardEnableEntry OBJECT-TYPE
| SYNTAX FtthPerformanceCardEnableEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { ftthPerformanceCardEnableTable 1 }
| FtthPerformanceCardEnableEntry ::=
| SEQUENCE {
| ftthPerformanceCardEnable
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.8.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.8.1.1.2
| ftthPerformanceCardEnable OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| " 0-disable 1-enable"
| ::= { ftthPerformanceCardEnableEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.8.2
| -- 1.3.6.1.4.1.5875.800.3.8.2
| ftthIsPerformanceSupport OBJECT-TYPE
| SYNTAX INTEGER
| {
| unsupport(0),
| support(1)
| }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description :
| 0:support
| 1:unsupport"
| ::= { ftthPerformance 2 }
| -- 1.3.6.1.4.1.5875.800.3.8.3
| -- 1.3.6.1.4.1.5875.800.3.8.3
| ftthPerformanceEnableFor5516 OBJECT-TYPE
| SYNTAX INTEGER
| {
| disable(0),
| enable(1)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description :
| 0:disable
| 1:enable"
| ::= { ftthPerformance 3 }
| -- 1.3.6.1.4.1.5875.800.3.8.6
| -- 1.3.6.1.4.1.5875.800.3.8.6
| ftthSystemPerformance OBJECT IDENTIFIER ::= { ftthPerformance 6 }
| -- 1.3.6.1.4.1.5875.800.3.8.6.1
| -- 1.3.6.1.4.1.5875.800.3.8.6.1
| utilization OBJECT IDENTIFIER ::= { ftthSystemPerformance 1 }
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.1
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.1
| cpuUtilization OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "cpu utilization"
| ::= { utilization 1 }
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.2
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.2
| memUtilization OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "mem utilization"
| ::= { utilization 2 }
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.3
| -- 1.3.6.1.4.1.5875.800.3.8.6.1.3
| currentTemperature OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "current Temperature"
| ::= { utilization 3 }
| ftthVlanTransmitPerformanceTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FtthVlanTransmitPerformanceEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { ftthPerformance 7 }
| ftthVlanTransmitPerformanceEntry OBJECT-TYPE
| SYNTAX FtthVlanTransmitPerformanceEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { vlanID, uplinkIndex }
| ::= { ftthVlanTransmitPerformanceTable 1 }
| FtthVlanTransmitPerformanceEntry ::= SEQUENCE {
| vlanID Integer32,
| framesUs Counter32,
| framesDs Counter32,
| octetsUs Counter32,
| octetsDs Counter32,
| discardsUs Counter64,
| discardsDs Counter64
| }
| vlanID OBJECT-TYPE
| SYNTAX Integer32 ( 1 .. 4096 )
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { ftthVlanTransmitPerformanceEntry 1 }
| framesUs OBJECT-TYPE
| SYNTAX Counter32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| Up transmit messages"
| ::= { ftthVlanTransmitPerformanceEntry 2 }
| framesDs OBJECT-TYPE
| SYNTAX Counter32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| down transmit messages"
| ::= { ftthVlanTransmitPerformanceEntry 3 }
| octetsUs OBJECT-TYPE
| SYNTAX Counter32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| Up transmit octets"
| ::= { ftthVlanTransmitPerformanceEntry 4 }
| octetsDs OBJECT-TYPE
| SYNTAX Counter32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| down transmit octets"
| ::= { ftthVlanTransmitPerformanceEntry 5 }
| discardsUs OBJECT-TYPE
| SYNTAX Counter64
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| up discards messages"
| ::= { ftthVlanTransmitPerformanceEntry 6 }
| discardsDs OBJECT-TYPE
| SYNTAX Counter64
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description
| down discards messages"
| ::= { ftthVlanTransmitPerformanceEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.9
| -- 1.3.6.1.4.1.5875.800.3.9
| systemInfo OBJECT IDENTIFIER ::= { oltData 9 }
| -- 1.3.6.1.4.1.5875.800.3.9.1
| -- 1.3.6.1.4.1.5875.800.3.9.1
| frameInfo OBJECT IDENTIFIER ::= { systemInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.1.1
| frameInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FrameInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { frameInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1
| frameInfoEntry OBJECT-TYPE
| SYNTAX FrameInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { frameIndex }
| ::= { frameInfoTable 1 }
| FrameInfoEntry ::=
| SEQUENCE {
| frameIndex
| Integer32,
| frameType
| Integer32,
| frameName
| OCTET STRING,
| slotNumOfFrame
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.1
| frameIndex OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { frameInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.2
| frameType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1: An5116-02
| 2: An5116-06
| 11: An5516-01 1"
| ::= { frameInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.3
| frameName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { frameInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.1.1.1.4
| slotNumOfFrame OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { frameInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.2
| -- 1.3.6.1.4.1.5875.800.3.9.2
| cardInfo OBJECT IDENTIFIER ::= { systemInfo 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1
| -- 1.3.6.1.4.1.5875.800.3.9.2.1
| cardInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF CardInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { cardInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1
| cardInfoEntry OBJECT-TYPE
| SYNTAX CardInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { cardInfoTable 1 }
| CardInfoEntry ::=
| SEQUENCE {
| cardType
| Integer32,
| cardHardwareVersion
| OCTET STRING,
| cardSoftwateVersion
| OCTET STRING,
| cardStatus
| Integer32,
| cardNumOfPorts
| Integer32,
| cardAvailablePorts
| Integer32,
| cardCpuUtil
| Integer32,
| cardMemUtil
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.2
| cardType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 260:EC2
| 724:EC2-X
| 16384:AC16
| the other type could see the card type table"
| ::= { cardInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.3
| cardHardwareVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { cardInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.4
| cardSoftwateVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { cardInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.5
| cardStatus OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:normal(1)
| 2:communication interrupt(0)"
| ::= { cardInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.6
| cardNumOfPorts OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { cardInfoEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.7
| cardAvailablePorts OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { cardInfoEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.8
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.8
| cardCpuUtil OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { cardInfoEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.9
| -- 1.3.6.1.4.1.5875.800.3.9.2.1.1.9
| cardMemUtil OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { cardInfoEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.9.3
| -- 1.3.6.1.4.1.5875.800.3.9.3
| interfaceInfo OBJECT IDENTIFIER ::= { systemInfo 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.1
| portInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PortInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1
| portInfoEntry OBJECT-TYPE
| SYNTAX PortInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { portInfoTable 1 }
| PortInfoEntry ::=
| SEQUENCE {
| portType
| Integer32,
| portEnableStatus
| Integer32,
| portOnlineStatus
| Integer32,
| portSpeed
| Integer32,
| portName
| OCTET STRING,
| portDesc
| OCTET STRING,
| portMode
| Integer32,
| portVlan
| OCTET STRING,
| portMac
| OCTET STRING,
| portDefaultVlan
| Integer32,
| portAutoneg
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.2
| portType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { portInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.3
| portEnableStatus OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "0-disable
| 1-enable"
| ::= { portInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.4
| portOnlineStatus OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.5
| portSpeed OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description:
| 0:10M
| 1:100M
| 2:1000M"
| ::= { portInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.6
| portName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.7
| portDesc OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.8
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.8
| portMode OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description:
| 1:full duplex(1)
| 2:half duplex(0)"
| ::= { portInfoEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.9
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.9
| portVlan OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.10
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.10
| portMac OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.11
| -- 1.3.6.1.4.1.5875.800.3.9.3.1.1.11
| portDefaultVlan OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { portInfoEntry 11 }
| portAutoneg OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 1 )
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { portInfoEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.2
| potsInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PotsInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1
| potsInfoEntry OBJECT-TYPE
| SYNTAX PotsInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { potsIndex }
| ::= { potsInfoTable 1 }
| PotsInfoEntry ::=
| SEQUENCE {
| potsType
| Integer32,
| potsName
| OCTET STRING,
| potsDesc
| OCTET STRING,
| potsEnableStatus
| Integer32,
| potsIdleStatus
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.1
| potsType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { potsInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.2
| potsName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { potsInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.3
| potsDesc OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { potsInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.4
| potsEnableStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:enable(1)
| 2:disable(2)"
| ::= { potsInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.2.1.5
| potsIdleStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { potsInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.3
| onuPonInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuPonInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1
| onuPonInfoEntry OBJECT-TYPE
| SYNTAX OnuPonInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onuPonInfoTable 1 }
| OnuPonInfoEntry ::=
| SEQUENCE {
| onuPonType
| Integer32,
| onuPonName
| OCTET STRING,
| onuPonDesc
| OCTET STRING,
| onuPonEnableStatus
| Integer32,
| onuPonSpeed
| Integer32,
| onuPonRxOpticalPower
| Integer32,
| onuPonTxOpticalPower
| Integer32,
| onuPonOpticalVltage
| Integer32,
| onuPonOpticalCurrent
| Integer32,
| onuPonOpticalTemperature
| Integer32,
| onuPonIsOpticalPowerValid
| INTEGER,
| onuPonUpstreamSpeed
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.1
| onuPonType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.2
| onuPonName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.3
| onuPonDesc OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.4
| onuPonEnableStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.5
| onuPonSpeed OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.6
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.6
| onuPonRxOpticalPower OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.7
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.7
| onuPonTxOpticalPower OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.8
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.8
| onuPonOpticalVltage OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.9
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.9
| onuPonOpticalCurrent OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.10
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.10
| onuPonOpticalTemperature OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonInfoEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.11
| -- 1.3.6.1.4.1.5875.800.3.9.3.3.1.11
| onuPonIsOpticalPowerValid OBJECT-TYPE
| SYNTAX INTEGER
| {
| support(1),
| nonsupport(2)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description:
| 1:support
| 2:nonsupport"
| ::= { onuPonInfoEntry 11 }
| onuPonUpstreamSpeed OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { onuPonInfoEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.4
| oltPonInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OltPonInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1
| oltPonInfoEntry OBJECT-TYPE
| SYNTAX OltPonInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { ponIndex }
| ::= { oltPonInfoTable 1 }
| OltPonInfoEntry ::=
| SEQUENCE {
| oltPonType
| Integer32,
| oltPonName
| OCTET STRING,
| oltPonDesc
| OCTET STRING,
| oltPonEnableStatus
| Integer32,
| oltPonOnlineStatus
| Integer32,
| oltPonSpeed
| Integer32,
| oltPonTxOpticalPower
| Integer32,
| oltPonOpticalVltage
| Integer32,
| oltPonOpticalCurrent
| Integer32,
| oltPonOpticalTemperature
| Integer32,
| oltPonAuthOnuNum
| Integer32,
| oltPonUpStreamSpeed
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.1
| oltPonType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.2
| oltPonName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.3
| oltPonDesc OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.4
| oltPonEnableStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.5
| oltPonOnlineStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:occupied(1)
| 2:empty(0)"
| ::= { oltPonInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.6
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.6
| oltPonSpeed OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| unit bps
| 0:10M
| 1:100M
| 2:1000M"
| ::= { oltPonInfoEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.8
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.8
| oltPonTxOpticalPower OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.9
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.9
| oltPonOpticalVltage OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.10
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.10
| oltPonOpticalCurrent OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.11
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.11
| oltPonOpticalTemperature OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonInfoEntry 11 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.12
| -- 1.3.6.1.4.1.5875.800.3.9.3.4.1.12
| oltPonAuthOnuNum OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { oltPonInfoEntry 12 }
| oltPonUpStreamSpeed OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { oltPonInfoEntry 13 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.5
| oltUplinkInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OltUplinkInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1
| oltUplinkInfoEntry OBJECT-TYPE
| SYNTAX OltUplinkInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { uplinkIndex }
| ::= { oltUplinkInfoTable 1 }
| OltUplinkInfoEntry ::=
| SEQUENCE {
| uplinkType
| Integer32,
| uplinkName
| OCTET STRING,
| uplinkDesc
| OCTET STRING,
| uplinkEnableStatus
| Integer32,
| uplinkSpeed
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.1
| uplinkType OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| AN5516_01B:
| 0:FE
| 1:GE
| 2:XGE /*10G*/
| 4:TRUNK"
| ::= { oltUplinkInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.2
| uplinkName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltUplinkInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.3
| uplinkDesc OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltUplinkInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.4
| uplinkEnableStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:enable(1)
| 2:disable(2)"
| ::= { oltUplinkInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.3.5.1.5
| uplinkSpeed OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| unit:bps"
| ::= { oltUplinkInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.6
| -- 1.3.6.1.4.1.5875.800.3.9.3.6
| oltPonOpticalStatisticsTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OltPonOpticalStatisticsEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { interfaceInfo 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.3.6.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.6.1
| oltPonopticalStatisticsEntry OBJECT-TYPE
| SYNTAX OltPonOpticalStatisticsEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { ponIndex }
| ::= { oltPonOpticalStatisticsTable 1 }
| OltPonOpticalStatisticsEntry ::=
| SEQUENCE {
| oltPonOpticalStatisticsSwitch
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.3.6.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.3.6.1.1
| oltPonOpticalStatisticsSwitch OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { oltPonopticalStatisticsEntry 1 }
| oltPonRxOpticalPowerTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OltPonRxOpticalPowerEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { interfaceInfo 7 }
| oltPonRxOpticalPowerEntry OBJECT-TYPE
| SYNTAX OltPonRxOpticalPowerEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { ponIndex, onuNoRxOpticalPower }
| ::= { oltPonRxOpticalPowerTable 1 }
| OltPonRxOpticalPowerEntry ::= SEQUENCE {
| onuNoRxOpticalPower Integer32,
| oltPonRxOpticalPower Integer32
| }
| onuNoRxOpticalPower OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { oltPonRxOpticalPowerEntry 1 }
| oltPonRxOpticalPower OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { oltPonRxOpticalPowerEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.4
| -- 1.3.6.1.4.1.5875.800.3.9.4
| sysInfo OBJECT IDENTIFIER ::= { systemInfo 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.4.1
| -- 1.3.6.1.4.1.5875.800.3.9.4.1
| sysIp OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sysInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.4.2
| -- 1.3.6.1.4.1.5875.800.3.9.4.2
| sysMac OBJECT-TYPE
| SYNTAX MacAddress
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sysInfo 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.4.3
| -- 1.3.6.1.4.1.5875.800.3.9.4.3
| sysSoftVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sysInfo 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.4.4
| -- 1.3.6.1.4.1.5875.800.3.9.4.4
| sysHardVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sysInfo 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.4.5
| -- 1.3.6.1.4.1.5875.800.3.9.4.5
| sysTemperature OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sysInfo 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.5
| -- 1.3.6.1.4.1.5875.800.3.9.5
| slotInfoFor5516 OBJECT IDENTIFIER ::= { systemInfo 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.5.1
| -- 1.3.6.1.4.1.5875.800.3.9.5.1
| slotInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF SlotInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { slotInfoFor5516 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1
| slotInfoEntry OBJECT-TYPE
| SYNTAX SlotInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { slotInfoTable 1 }
| SlotInfoEntry ::=
| SEQUENCE {
| occupiedStatus
| INTEGER,
| authCardType
| Integer32,
| occupiedCardType
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.2
| occupiedStatus OBJECT-TYPE
| SYNTAX INTEGER
| {
| occupied(1),
| empty(0)
| }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:occupied(1)
| 2:empty(0)"
| ::= { slotInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.3
| authCardType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { slotInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.5.1.1.4
| occupiedCardType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { slotInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.6
| -- 1.3.6.1.4.1.5875.800.3.9.6
| onu2PonLength OBJECT IDENTIFIER ::= { systemInfo 6 }
| -- 1.3.6.1.4.1.5875.800.3.9.6.1
| -- 1.3.6.1.4.1.5875.800.3.9.6.1
| onu2PonLengthTable OBJECT-TYPE
| SYNTAX SEQUENCE OF Onu2PonLengthEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onu2PonLength 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.6.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.6.1.1
| onu2PonLengthEntry OBJECT-TYPE
| SYNTAX Onu2PonLengthEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onu2PonLengthTable 1 }
| Onu2PonLengthEntry ::=
| SEQUENCE {
| length
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.6.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.6.1.1.1
| length OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description:
| need the onu online, otherwise the length will be zero"
| ::= { onu2PonLengthEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.8
| -- 1.3.6.1.4.1.5875.800.3.9.8
| mgrCardInfo OBJECT IDENTIFIER ::= { systemInfo 8 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1
| -- 1.3.6.1.4.1.5875.800.3.9.8.1
| mgrCardInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF MgrCardInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { mgrCardInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1
| mgrCardInfoEntry OBJECT-TYPE
| SYNTAX MgrCardInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { mgrCardInfoTable 1 }
| MgrCardInfoEntry ::=
| SEQUENCE {
| mgrCardType
| Integer32,
| mgrCardHandwareVersion
| OCTET STRING,
| mgrCardSoftwareVession
| OCTET STRING,
| mgrCardWorkStatus
| Integer32,
| mgrCardCpuUtil
| Integer32,
| mgrCardMemUtil
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.1
| mgrCardType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description
| 1:normal(1)
| 2:communication interrupt(0)"
| ::= { mgrCardInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.2
| mgrCardHandwareVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mgrCardInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.3
| mgrCardSoftwareVession OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mgrCardInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.4
| mgrCardWorkStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mgrCardInfoEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.5
| mgrCardCpuUtil OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mgrCardInfoEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.9.8.1.1.6
| mgrCardMemUtil OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mgrCardInfoEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.10
| -- 1.3.6.1.4.1.5875.800.3.10
| authOnuInf OBJECT IDENTIFIER ::= { oltData 10 }
| -- 1.3.6.1.4.1.5875.800.3.10.1
| -- 1.3.6.1.4.1.5875.800.3.10.1
| authOnuListTable OBJECT-TYPE
| SYNTAX SEQUENCE OF AuthOnuListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { authOnuInf 1 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1
| -- 1.3.6.1.4.1.5875.800.3.10.1.1
| authOnuListEntry OBJECT-TYPE
| SYNTAX AuthOnuListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { authOnuListTable 1 }
| AuthOnuListEntry ::=
| SEQUENCE {
| authOnuListSlot
| Integer32,
| authOnuListPon
| Integer32,
| authOnuListOnuid
| Integer32,
| authOnuListOnuType
| Integer32,
| authOnuListIp
| OCTET STRING,
| authOnuListName
| OCTET STRING,
| authOnuListSnLoid
| OCTET STRING,
| authOnuListSnPwd
| OCTET STRING,
| authOnuListMac
| OCTET STRING,
| onuStatus
| Integer32,
| authOnuSoftwareVersion
| OCTET STRING,
| authOnuHardwareVersion
| OCTET STRING,
| authOnuFirmwareVersion
| OCTET STRING
| }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.2
| authOnuListSlot OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.3
| authOnuListPon OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.4
| authOnuListOnuid OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.5
| authOnuListOnuType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.6
| authOnuListIp OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.7
| authOnuListName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.8
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.8
| authOnuListSnLoid OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.9
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.9
| authOnuListSnPwd OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.10
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.10
| authOnuListMac OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { authOnuListEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.11
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.11
| onuStatus OBJECT-TYPE
| SYNTAX Integer32 (0..1)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description:
| 1:offonline/fiber cut/power failure(0)
| 2:online(1)"
| ::= { authOnuListEntry 11 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.12
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.12
| authOnuSoftwareVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { authOnuListEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.13
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.13
| authOnuHardwareVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { authOnuListEntry 13 }
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.14
| -- 1.3.6.1.4.1.5875.800.3.10.1.1.14
| authOnuFirmwareVersion OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { authOnuListEntry 14 }
| -- 1.3.6.1.4.1.5875.800.3.11
| -- 1.3.6.1.4.1.5875.800.3.11
| unauthOnuList OBJECT IDENTIFIER ::= { oltData 11 }
| -- 1.3.6.1.4.1.5875.800.3.11.1
| -- 1.3.6.1.4.1.5875.800.3.11.1
| unauthOnuListTable OBJECT-TYPE
| SYNTAX SEQUENCE OF UnauthOnuListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { unauthOnuList 1 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1
| -- 1.3.6.1.4.1.5875.800.3.11.1.1
| unauthOnuListEntry OBJECT-TYPE
| SYNTAX UnauthOnuListEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { unauthOnuListOnuIndex }
| ::= { unauthOnuListTable 1 }
| UnauthOnuListEntry ::=
| SEQUENCE {
| unauthOnuListOnuIndex
| Integer32,
| unauthOnuListSlot
| Integer32,
| unauthOnuListPon
| Integer32,
| unauthOnuListOnuType
| Integer32,
| unauthOnuListSnLoid
| OCTET STRING,
| unauthOnuListPwd
| OCTET STRING,
| unauthOnuListMac
| OCTET STRING
| }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.1
| unauthOnuListOnuIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.2
| unauthOnuListSlot OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.3
| unauthOnuListPon OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.4
| unauthOnuListOnuType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.5
| unauthOnuListSnLoid OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.6
| unauthOnuListPwd OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.11.1.1.7
| unauthOnuListMac OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { unauthOnuListEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.12
| -- 1.3.6.1.4.1.5875.800.3.12
| onuAuthModeFor5116 OBJECT IDENTIFIER ::= { oltData 12 }
| -- 1.3.6.1.4.1.5875.800.3.12.1
| -- 1.3.6.1.4.1.5875.800.3.12.1
| onuAuthModeTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuAuthModeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuAuthModeFor5116 1 }
| -- 1.3.6.1.4.1.5875.800.3.12.1.1
| -- 1.3.6.1.4.1.5875.800.3.12.1.1
| onuAuthModeEntry OBJECT-TYPE
| SYNTAX OnuAuthModeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { onuAuthModeTable 1 }
| OnuAuthModeEntry ::=
| SEQUENCE {
| macAuthEnable
| TruthValue,
| snAuthEnable
| TruthValue
| }
| -- 1.3.6.1.4.1.5875.800.3.12.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.12.1.1.2
| macAuthEnable OBJECT-TYPE
| SYNTAX TruthValue
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuAuthModeEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.12.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.12.1.1.3
| snAuthEnable OBJECT-TYPE
| SYNTAX TruthValue
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuAuthModeEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.13
| -- 1.3.6.1.4.1.5875.800.3.13
| onuWarrantTypeFor5116 OBJECT IDENTIFIER ::= { oltData 13 }
| -- 1.3.6.1.4.1.5875.800.3.13.1
| -- 1.3.6.1.4.1.5875.800.3.13.1
| onuWarrentTypeTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuWarrentTypeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuWarrantTypeFor5116 1 }
| -- 1.3.6.1.4.1.5875.800.3.13.1.1
| -- 1.3.6.1.4.1.5875.800.3.13.1.1
| onuWarrentTypeEntry OBJECT-TYPE
| SYNTAX OnuWarrentTypeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { onuWarrentTypeTable 1 }
| OnuWarrentTypeEntry ::=
| SEQUENCE {
| warrantType
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.13.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.13.1.1.2
| warrantType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuWarrentTypeEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.14
| -- 1.3.6.1.4.1.5875.800.3.14
| ponAuthModeFor5516 OBJECT IDENTIFIER ::= { oltData 14 }
| -- 1.3.6.1.4.1.5875.800.3.14.1
| -- 1.3.6.1.4.1.5875.800.3.14.1
| ponAuthModeTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PonAuthModeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { ponAuthModeFor5516 1 }
| -- 1.3.6.1.4.1.5875.800.3.14.1.1
| -- 1.3.6.1.4.1.5875.800.3.14.1.1
| ponAuthModeEntry OBJECT-TYPE
| SYNTAX PonAuthModeEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { ponIndex }
| ::= { ponAuthModeTable 1 }
| PonAuthModeEntry ::=
| SEQUENCE {
| authMode
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.14.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.14.1.1.2
| authMode OBJECT-TYPE
| SYNTAX Integer32 (0..8)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 0:Physical Markup authentication
| 1:Physical Markup +Physical password authentication
| 2:Physical password authentication
| 3:Logic Markup +Logic password authentication
| 4:Physical Markup /Logic Markup(include password)mix authentication
| 5:unauthentication
| 6:Logic Markup authentication(except password)
| 7:Physical Markup /Logic Markup(except password)mix authentication
| 8:Logic password authentication"
| ::= { ponAuthModeEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.15
| -- 1.3.6.1.4.1.5875.800.3.15
| cardWarrentFor5516 OBJECT IDENTIFIER ::= { oltData 15 }
| -- 1.3.6.1.4.1.5875.800.3.15.1
| -- 1.3.6.1.4.1.5875.800.3.15.1
| cardWarrentTable OBJECT-TYPE
| SYNTAX SEQUENCE OF CardWarrentEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { cardWarrentFor5516 1 }
| -- 1.3.6.1.4.1.5875.800.3.15.1.1
| -- 1.3.6.1.4.1.5875.800.3.15.1.1
| cardWarrentEntry OBJECT-TYPE
| SYNTAX CardWarrentEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { cardWarrentTable 1 }
| CardWarrentEntry ::=
| SEQUENCE {
| warrentCardType
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.15.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.15.1.1.2
| warrentCardType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { cardWarrentEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.16
| -- 1.3.6.1.4.1.5875.800.3.16
| globalVlan OBJECT IDENTIFIER ::= { oltData 16 }
| -- 1.3.6.1.4.1.5875.800.3.16.1
| -- 1.3.6.1.4.1.5875.800.3.16.1
| globalVlanTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GlobalVlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { globalVlan 1 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1
| -- 1.3.6.1.4.1.5875.800.3.16.1.1
| globalVlanEntry OBJECT-TYPE
| SYNTAX GlobalVlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { vlanConfigId }
| ::= { globalVlanTable 1 }
| GlobalVlanEntry ::=
| SEQUENCE {
| vlanConfigId
| Integer32,
| serviceName
| OCTET STRING,
| beginVlanId
| Integer32,
| endVlanId
| Integer32,
| upLinkPort
| Integer32,
| tagStatus
| INTEGER,
| globalVlanAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.1
| vlanConfigId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.2
| serviceName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.3
| beginVlanId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.4
| endVlanId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.5
| upLinkPort OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.6
| tagStatus OBJECT-TYPE
| SYNTAX INTEGER
| {
| tag(1),
| untag(0)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:tag(1)
| 2:untag(0)"
| ::= { globalVlanEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.16.1.1.7
| globalVlanAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { globalVlanEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.16.2
| -- 1.3.6.1.4.1.5875.800.3.16.2
| nextGlobalVlanId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { globalVlan 2 }
| -- 1.3.6.1.4.1.5875.800.3.17
| -- 1.3.6.1.4.1.5875.800.3.17
| onuManageVlan OBJECT IDENTIFIER ::= { oltData 17 }
| -- 1.3.6.1.4.1.5875.800.3.17.1
| -- 1.3.6.1.4.1.5875.800.3.17.1
| onuManageVlanTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuManageVlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuManageVlan 1 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1
| -- 1.3.6.1.4.1.5875.800.3.17.1.1
| onuManageVlanEntry OBJECT-TYPE
| SYNTAX OnuManageVlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex , manageVlanIndex }
| ::= { onuManageVlanTable 1 }
| OnuManageVlanEntry ::=
| SEQUENCE {
| manageVlanIndex
| Integer32,
| onuMac
| MacAddress,
| manageVlanName
| OCTET STRING,
| portNo
| Integer32,
| tagStatus1
| Integer32,
| manageSvlan
| Integer32,
| manageSvlanCos
| Integer32,
| mamageCvlan
| Integer32,
| mamageCvlanCos
| Integer32,
| onuIp
| IpAddress,
| onuMask
| IpAddress,
| onuGateway
| IpAddress,
| onuManageVlanAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.2
| manageVlanIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 1 }
| onuMac OBJECT-TYPE
| SYNTAX MacAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.4
| manageVlanName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.5
| portNo OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.6
| tagStatus1 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.7
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.7
| manageSvlan OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 7 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.8
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.8
| manageSvlanCos OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 8 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.9
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.9
| mamageCvlan OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.10
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.10
| mamageCvlanCos OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 10 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.11
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.11
| onuIp OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 11 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.12
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.12
| onuMask OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 12 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.13
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.13
| onuGateway OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 13 }
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.14
| -- 1.3.6.1.4.1.5875.800.3.17.1.1.14
| onuManageVlanAction OBJECT-TYPE
| SYNTAX INTEGER { modify(7) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuManageVlanEntry 14 }
| -- 1.3.6.1.4.1.5875.800.3.18
| -- 1.3.6.1.4.1.5875.800.3.18
| trunkConfig OBJECT IDENTIFIER ::= { oltData 18 }
| -- 1.3.6.1.4.1.5875.800.3.18.1
| -- 1.3.6.1.4.1.5875.800.3.18.1
| trunkConfigTable OBJECT-TYPE
| SYNTAX SEQUENCE OF TrunkConfigEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { trunkConfig 1 }
| -- 1.3.6.1.4.1.5875.800.3.18.1.1
| -- 1.3.6.1.4.1.5875.800.3.18.1.1
| trunkConfigEntry OBJECT-TYPE
| SYNTAX TrunkConfigEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { trunkGroupId }
| ::= { trunkConfigTable 1 }
| TrunkConfigEntry ::=
| SEQUENCE {
| trunkGroupId
| Integer32,
| masterPort
| Integer32,
| memberPort
| Integer32,
| trunkConfigAction
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.1
| trunkGroupId OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { trunkConfigEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.2
| masterPort OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { trunkConfigEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.3
| memberPort OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "ctp,<<=127; ?nit +?Xb 1-7;"
| ::= { trunkConfigEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.18.1.1.4
| trunkConfigAction OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6),
| modify(7)
| }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { trunkConfigEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.18.2
| -- 1.3.6.1.4.1.5875.800.3.18.2
| nextTrunkConfigId OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { trunkConfig 2 }
| -- 1.3.6.1.4.1.5875.800.3.19
| -- 1.3.6.1.4.1.5875.800.3.19
| onuPonConfig OBJECT IDENTIFIER ::= { oltData 19 }
| -- 1.3.6.1.4.1.5875.800.3.19.1
| -- 1.3.6.1.4.1.5875.800.3.19.1
| onuPonCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuPonCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPonConfig 1 }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1
| -- 1.3.6.1.4.1.5875.800.3.19.1.1
| onuPonCfgEntry OBJECT-TYPE
| SYNTAX OnuPonCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onuPonCfgTable 1 }
| OnuPonCfgEntry ::=
| SEQUENCE {
| upBandwidth
| Integer32,
| dnBandwidth
| Integer32,
| upAssureBandwidth
| Integer32,
| upFixedBandwidth
| Integer32,
| onuPonCfgActon
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.1
| upBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonCfgEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.2
| dnBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPonCfgEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.3
| upAssureBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPonCfgEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.4
| upFixedBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPonCfgEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.19.1.1.5
| onuPonCfgActon OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuPonCfgEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.20
| -- 1.3.6.1.4.1.5875.800.3.20
| saveCfg2Flash OBJECT IDENTIFIER ::= { oltData 20 }
| -- 1.3.6.1.4.1.5875.800.3.20.1
| -- 1.3.6.1.4.1.5875.800.3.20.1
| save2Flash OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { saveCfg2Flash 1 }
| -- 1.3.6.1.4.1.5875.800.3.21
| -- 1.3.6.1.4.1.5875.800.3.21
| mac2OnuInfo OBJECT IDENTIFIER ::= { oltData 21 }
| -- 1.3.6.1.4.1.5875.800.3.21.1
| -- 1.3.6.1.4.1.5875.800.3.21.1
| mac2OnuInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF Mac2OnuInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { mac2OnuInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.21.1.1
| -- 1.3.6.1.4.1.5875.800.3.21.1.1
| mac2OnuInfoEntry OBJECT-TYPE
| SYNTAX Mac2OnuInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuMacString }
| ::= { mac2OnuInfoTable 1 }
| Mac2OnuInfoEntry ::=
| SEQUENCE {
| onuMacString
| OCTET STRING,
| onuAuthID
| Integer32,
| onuWhileListID
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.1
| onuMacString OBJECT-TYPE
| SYNTAX OCTET STRING (SIZE (12))
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mac2OnuInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.2
| onuAuthID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mac2OnuInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.21.1.1.3
| onuWhileListID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { mac2OnuInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.22
| -- 1.3.6.1.4.1.5875.800.3.22
| sn2OnuInfo OBJECT IDENTIFIER ::= { oltData 22 }
| -- 1.3.6.1.4.1.5875.800.3.22.1
| -- 1.3.6.1.4.1.5875.800.3.22.1
| sn2OnuInfoTable OBJECT-TYPE
| SYNTAX SEQUENCE OF Sn2OnuInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { sn2OnuInfo 1 }
| -- 1.3.6.1.4.1.5875.800.3.22.1.1
| -- 1.3.6.1.4.1.5875.800.3.22.1.1
| sn2OnuInfoEntry OBJECT-TYPE
| SYNTAX Sn2OnuInfoEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuSNString }
| ::= { sn2OnuInfoTable 1 }
| Sn2OnuInfoEntry ::=
| SEQUENCE {
| onuSNString
| OCTET STRING,
| onuSNAuthID
| Integer32,
| onuSNWhilteListID
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.1
| onuSNString OBJECT-TYPE
| SYNTAX OCTET STRING (SIZE (1..24))
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { sn2OnuInfoEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.2
| onuSNAuthID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { sn2OnuInfoEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.22.1.1.3
| onuSNWhilteListID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { sn2OnuInfoEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.23
| -- 1.3.6.1.4.1.5875.800.3.23
| snmpConfig OBJECT IDENTIFIER ::= { oltData 23 }
| -- 1.3.6.1.4.1.5875.800.3.23.1
| -- 1.3.6.1.4.1.5875.800.3.23.1
| trapReceiveIp OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { snmpConfig 1 }
| -- 1.3.6.1.4.1.5875.800.3.23.2
| -- 1.3.6.1.4.1.5875.800.3.23.2
| community OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Description"
| ::= { snmpConfig 2 }
| snmpTrapTable OBJECT-TYPE
| SYNTAX SEQUENCE OF SnmpTrapEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { snmpConfig 3 }
| snmpTrapEntry OBJECT-TYPE
| SYNTAX SnmpTrapEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { snmpTrapIndex }
| ::= { snmpTrapTable 1 }
| SnmpTrapEntry ::= SEQUENCE {
| snmpTrapIndex Integer32,
| snmpTrapIpv4 IpAddress,
| snmpTrapPort Integer32,
| snmpTrapVersion INTEGER,
| snmpTrapReportVersion INTEGER,
| snmpTrapCommunity OCTET STRING,
| snmpTrapAction INTEGER
| }
| snmpTrapIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 1 }
| snmpTrapIpv4 OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 2 }
| snmpTrapPort OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 3 }
| snmpTrapVersion OBJECT-TYPE
| SYNTAX INTEGER { v1 ( 1 ) , v2c ( 2 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 4 }
| snmpTrapReportVersion OBJECT-TYPE
| SYNTAX INTEGER { privFormat ( 0 ) , stdFormat ( 1 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 5 }
| snmpTrapCommunity OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 6 }
| snmpTrapAction OBJECT-TYPE
| SYNTAX INTEGER { create ( 4 ) , destroy ( 6 ) , modify ( 7 ) , active ( 1 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpTrapEntry 20 }
| snmpCommunityTable OBJECT-TYPE
| SYNTAX SEQUENCE OF SnmpCommunityEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { snmpConfig 4 }
| snmpCommunityEntry OBJECT-TYPE
| SYNTAX SnmpCommunityEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { snmpCommunityIndex }
| ::= { snmpCommunityTable 1 }
| SnmpCommunityEntry ::= SEQUENCE {
| snmpCommunityIndex Integer32,
| snmpCommunity OCTET STRING,
| snmpCommunityPermission INTEGER
| }
| snmpCommunityIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpCommunityEntry 1 }
| snmpCommunity OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpCommunityEntry 2 }
| snmpCommunityPermission OBJECT-TYPE
| SYNTAX INTEGER { ro ( 1 ) , rw ( 2 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { snmpCommunityEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.24
| -- 1.3.6.1.4.1.5875.800.3.24
| igmpConfig OBJECT IDENTIFIER ::= { oltData 24 }
| igmpBaseCfg OBJECT IDENTIFIER
| ::= { igmpConfig 1 }
| igmpMode OBJECT-TYPE
| SYNTAX INTEGER { controlled ( 1 ) , proxy-proxy ( 2 ) , snooping ( 3 ) , proxy-snooping ( 4 ) , disable ( 5 ) , active ( 6 ) }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpBaseCfg 1 }
| igmpVlan OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpBaseCfg 2 }
| igmpProxyIp OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpBaseCfg 3 }
| igmpProtocolVersion OBJECT-TYPE
| SYNTAX INTEGER { igmpv1v2 ( 1 ) , igmpv3 ( 2 ) }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpBaseCfg 4 }
| igmpProtocolPara OBJECT IDENTIFIER
| ::= { igmpConfig 2 }
| robustnessVariable OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 1 }
| queryRespInterval OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 2 }
| lastQueryInterval OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 3 }
| lastQueryCount OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 4 }
| queryInterval OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 5 }
| groupMembInterval OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpProtocolPara 6 }
| igmpProfileTable OBJECT-TYPE
| SYNTAX SEQUENCE OF IgmpProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpConfig 4 }
| igmpProfileEntry OBJECT-TYPE
| SYNTAX IgmpProfileEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { igmpProfileIndex }
| ::= { igmpProfileTable 1 }
| IgmpProfileEntry ::= SEQUENCE {
| igmpProfileIndex Integer32,
| igmpProfileName OCTET STRING,
| igmpProfileAction INTEGER
| }
| igmpProfileIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileEntry 1 }
| igmpProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileEntry 2 }
| igmpProfileAction OBJECT-TYPE
| SYNTAX INTEGER { active ( 1 ) , create ( 4 ) , destroy ( 6 ) , modify ( 7 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileEntry 20 }
| igmpProfileGroupTable OBJECT-TYPE
| SYNTAX SEQUENCE OF IgmpProfileGroupEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpConfig 5 }
| igmpProfileGroupEntry OBJECT-TYPE
| SYNTAX IgmpProfileGroupEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { igmpProfileIndex, igmpProfileGroupIndex }
| ::= { igmpProfileGroupTable 1 }
| IgmpProfileGroupEntry ::= SEQUENCE {
| igmpProfileGroupIndex Integer32,
| groupAddressBegin IpAddress,
| groupAddressEnd IpAddress,
| igmpProfileGroupAuthority INTEGER,
| igmpProfileGroupAction INTEGER
| }
| igmpProfileGroupIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileGroupEntry 1 }
| groupAddressBegin OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileGroupEntry 2 }
| groupAddressEnd OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileGroupEntry 3 }
| igmpProfileGroupAuthority OBJECT-TYPE
| SYNTAX INTEGER { normal ( 1 ) , preview ( 2 ) , forbid ( 3 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileGroupEntry 4 }
| igmpProfileGroupAction OBJECT-TYPE
| SYNTAX INTEGER { active ( 1 ) , create ( 4 ) , destroy ( 6 ) , modify ( 7 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpProfileGroupEntry 20 }
| igmpActiveMultiGroupNumberTable OBJECT-TYPE
| SYNTAX SEQUENCE OF IgmpActiveMultiGroupNumberEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpConfig 6 }
| igmpActiveMultiGroupNumberEntry OBJECT-TYPE
| SYNTAX IgmpActiveMultiGroupNumberEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { portIndex, igmpvlan }
| ::= { igmpActiveMultiGroupNumberTable 1 }
| IgmpActiveMultiGroupNumberEntry ::= SEQUENCE {
| igmpvlan Integer32,
| igmpActiveMultiGroup Integer32
| }
| igmpvlan OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpActiveMultiGroupNumberEntry 1 }
| igmpActiveMultiGroup OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpActiveMultiGroupNumberEntry 2 }
| igmpactiveJoinPortsNumberTable OBJECT-TYPE
| SYNTAX SEQUENCE OF IgmpactiveJoinPortsNumberEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpConfig 7 }
| igmpactiveJoinPortsNumberEntry OBJECT-TYPE
| SYNTAX IgmpactiveJoinPortsNumberEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { fttbIfIndex, igmpMultiGroupAddress }
| ::= { igmpactiveJoinPortsNumberTable 1 }
| IgmpactiveJoinPortsNumberEntry ::= SEQUENCE {
| igmpMultiGroupAddress IpAddress,
| activeJoinPorts Integer32
| }
| igmpMultiGroupAddress OBJECT-TYPE
| SYNTAX IpAddress
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpactiveJoinPortsNumberEntry 1 }
| activeJoinPorts OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { igmpactiveJoinPortsNumberEntry 2 }
| portIgmpCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PortIgmpCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { igmpConfig 8 }
| portIgmpCfgEntry OBJECT-TYPE
| SYNTAX PortIgmpCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { portIndex, profileIndex }
| ::= { portIgmpCfgTable 1 }
| PortIgmpCfgEntry ::= SEQUENCE {
| profileIndex Integer32,
| portCtrlEnable INTEGER,
| igmpProfile OCTET STRING,
| leaveMode INTEGER,
| maxOnlineNum Integer32,
| portBandwidth Integer32,
| portSignalVlan Integer32,
| portIgmpCfgAction RowStatus
| }
| profileIndex OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { portIgmpCfgEntry 1 }
| portCtrlEnable OBJECT-TYPE
| SYNTAX INTEGER { controlled ( 1 ) , uncontrolled ( 0 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 2 }
| igmpProfile OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 3 }
| leaveMode OBJECT-TYPE
| SYNTAX INTEGER { nonFastLeave ( 0 ) , fastLeave ( 1 ) }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 4 }
| maxOnlineNum OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 5 }
| portBandwidth OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 6 }
| portSignalVlan OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 7 }
| portIgmpCfgAction OBJECT-TYPE
| SYNTAX RowStatus { active ( 1 ) , notInService ( 2 ) , notReady ( 3 ) , createAndGo ( 4 ) , createAndWait ( 5 ) , destroy ( 6 ) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION "Column Description"
| ::= { portIgmpCfgEntry 20 }
| -- 1.3.6.1.4.1.5875.800.3.25
| -- 1.3.6.1.4.1.5875.800.3.25
| onuAuth OBJECT IDENTIFIER ::= { oltData 25 }
| -- 1.3.6.1.4.1.5875.800.3.25.1
| -- 1.3.6.1.4.1.5875.800.3.25.1
| onuPhysicsAuthTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuPhysicsAuthEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuAuth 1 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1
| -- 1.3.6.1.4.1.5875.800.3.25.1.1
| onuPhysicsAuthEntry OBJECT-TYPE
| SYNTAX OnuPhysicsAuthEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onuPhysicsAuthTable 1 }
| OnuPhysicsAuthEntry ::=
| SEQUENCE {
| onuSlotForMacAuth
| Integer32,
| onuPonForMacAuth
| Integer32,
| onuNoForMacAuth
| Integer32,
| onuTypeForMacAuth
| Integer32,
| macForMacAuth
| OCTET STRING,
| passwordForMacAuth
| OCTET STRING,
| actionForMacAuth
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.1
| onuSlotForMacAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.2
| onuPonForMacAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.3
| onuNoForMacAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.4
| onuTypeForMacAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.5
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.5
| macForMacAuth OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 5 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.6
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.6
| passwordForMacAuth OBJECT-TYPE
| SYNTAX OCTET STRING (SIZE (1..6))
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 6 }
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.17
| -- 1.3.6.1.4.1.5875.800.3.25.1.1.17
| actionForMacAuth OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuPhysicsAuthEntry 17 }
| -- 1.3.6.1.4.1.5875.800.3.25.2
| -- 1.3.6.1.4.1.5875.800.3.25.2
| onuSnAuthFor5116Table OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuSnAuthFor5116Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { onuAuth 2 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1
| -- 1.3.6.1.4.1.5875.800.3.25.2.1
| onuSnAuthFor5116Entry OBJECT-TYPE
| SYNTAX OnuSnAuthFor5116Entry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onuSnAuthFor5116Table 1 }
| OnuSnAuthFor5116Entry ::=
| SEQUENCE {
| slotNoForSnAuth
| Integer32,
| ponNoForSnMacAuth
| Integer32,
| onuNoForSnAuth
| Integer32,
| onuTypeForSnAuth
| Integer32,
| snForsnAuth
| OCTET STRING,
| passwordForSnAuth
| OCTET STRING,
| actionForSnAuth
| INTEGER
| }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.1
| slotNoForSnAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 1 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.2
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.2
| ponNoForSnMacAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 2 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.3
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.3
| onuNoForSnAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 3 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.4
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.4
| onuTypeForSnAuth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 4 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.5
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.5
| snForsnAuth OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 5 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.6
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.6
| passwordForSnAuth OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuSnAuthFor5116Entry 6 }
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.17
| -- 1.3.6.1.4.1.5875.800.3.25.2.1.17
| actionForSnAuth OBJECT-TYPE
| SYNTAX INTEGER
| {
| active(1),
| create(4),
| destroy(6)
| }
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description :
| 1:create(4)
| 2:destroy(6)"
| ::= { onuSnAuthFor5116Entry 17 }
| cvlan2Svlan OBJECT IDENTIFIER
| ::= { oltData 26 }
| cvlan2SvlanTable OBJECT-TYPE
| SYNTAX SEQUENCE OF Cvlan2SvlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { cvlan2Svlan 1 }
| cvlan2SvlanEntry OBJECT-TYPE
| SYNTAX Cvlan2SvlanEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { onuIndex, onuCvlanVid }
| ::= { cvlan2SvlanTable 1 }
| Cvlan2SvlanEntry ::= SEQUENCE {
| onuCvlanVid Integer32,
| onuSvlanVid Integer32
| }
| onuCvlanVid OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { cvlan2SvlanEntry 1 }
| onuSvlanVid OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Description"
| ::= { cvlan2SvlanEntry 2 }
| gponOnuServiceConfig OBJECT IDENTIFIER
| ::= { oltData 30 }
| -- 1.3.6.1.4.1.5875.800.3.50
| -- 1.3.6.1.4.1.5875.800.3.50
| gponConfig OBJECT IDENTIFIER ::= { oltData 50 }
| gponRmtManageCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GponRmtManageCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { gponOnuServiceConfig 1 }
| gponRmtManageCfgEntry OBJECT-TYPE
| SYNTAX GponRmtManageCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { onuIndex }
| ::= { gponRmtManageCfgTable 1 }
| GponRmtManageCfgEntry ::= SEQUENCE {
| gponRmtManageUrl OCTET STRING,
| gponRmtManageUser OCTET STRING,
| gponRmtManagePwd OCTET STRING,
| gponRmtManageAction INTEGER
| }
| gponRmtManageUrl OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponRmtManageCfgEntry 1 }
| gponRmtManageUser OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponRmtManageCfgEntry 2 }
| gponRmtManagePwd OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponRmtManageCfgEntry 3 }
| gponRmtManageAction OBJECT-TYPE
| SYNTAX INTEGER { active ( 1 ) , create ( 4 ) , modify ( 7 ) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION "Description"
| ::= { gponRmtManageCfgEntry 4 }
| gponVEIPManagePathCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GponVEIPManagePathCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { gponOnuServiceConfig 2 }
| gponVEIPManagePathCfgEntry OBJECT-TYPE
| SYNTAX GponVEIPManagePathCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { portIndex }
| ::= { gponVEIPManagePathCfgTable 1 }
| GponVEIPManagePathCfgEntry ::= SEQUENCE {
| gponVEIPManagePathDsp Integer32,
| gponVEIPManagePathIPAddress OCTET STRING,
| gponVEIPManagePathIpMask Integer32,
| gponVEIPManagePathGateWay OCTET STRING,
| gponVEIPManagePathPrimaryDns OCTET STRING,
| gponVEIPManagePathSecondaryDns OCTET STRING,
| gponVEIPManagePathNetworkPort Integer32,
| gponVEIPManagePathCVlan Integer32,
| gponVEIPManagePathCVlanCos Integer32,
| gponVEIPManagePathAction INTEGER
| }
| gponVEIPManagePathDsp OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 1 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 1 }
| gponVEIPManagePathIPAddress OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 2 }
| gponVEIPManagePathGateWay OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 3 }
| gponVEIPManagePathPrimaryDns OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 4 }
| gponVEIPManagePathSecondaryDns OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Description"
| ::= { gponVEIPManagePathCfgEntry 5 }
| gponVEIPManagePathNetworkPort OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 6 }
| gponVEIPManagePathCVlan OBJECT-TYPE
| SYNTAX Integer32 ( 1 .. 4085 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 7 }
| gponVEIPManagePathCVlanCos OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 7 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 8 }
| gponVEIPManagePathIpMask OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPManagePathCfgEntry 9 }
| gponVEIPManagePathAction OBJECT-TYPE
| SYNTAX INTEGER { active ( 1 ) , create ( 4 ) , destroy ( 6 ) , modify ( 7 ) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION "Description"
| ::= { gponVEIPManagePathCfgEntry 30 }
| gponVEIPServiceCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GponVEIPServiceCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { gponOnuServiceConfig 3 }
| gponVEIPServiceCfgEntry OBJECT-TYPE
| SYNTAX GponVEIPServiceCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { portIndex, gponVEIPServiceID }
| ::= { gponVEIPServiceCfgTable 1 }
| GponVEIPServiceCfgEntry ::= SEQUENCE {
| gponVEIPServiceID Integer32,
| gponVEIPServiceTls Integer32,
| gponVEIPServiceCVlan Integer32,
| gponVEIPServiceCVlanCos Integer32,
| gponVEIPServiceTVlan Integer32,
| gponVEIPServiceTVlanCos Integer32,
| gponVEIPServiceSVlan Integer32,
| gponVEIPServiceSVlanCos Integer32,
| gponVEIPServiceUsBandWidth Integer32,
| gponVEIPServiceDsBandWidth Integer32,
| gponVEIPServiceProfileName OCTET STRING,
| gponVEIPServiceAction INTEGER
| }
| gponVEIPServiceID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 1 }
| gponVEIPServiceTls OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 1 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 2 }
| gponVEIPServiceCVlan OBJECT-TYPE
| SYNTAX Integer32 ( 1 .. 4085 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 3 }
| gponVEIPServiceCVlanCos OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 7 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 4 }
| gponVEIPServiceTVlan OBJECT-TYPE
| SYNTAX Integer32 ( 1 .. 4085 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 5 }
| gponVEIPServiceTVlanCos OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 7 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 6 }
| gponVEIPServiceSVlan OBJECT-TYPE
| SYNTAX Integer32 ( 1 .. 4085 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 7 }
| gponVEIPServiceSVlanCos OBJECT-TYPE
| SYNTAX Integer32 ( 0 .. 7 | 65535 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 8 }
| gponVEIPServiceUsBandWidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 9 }
| gponVEIPServiceDsBandWidth OBJECT-TYPE
| SYNTAX Integer32 ( -2147483648 .. 2147483647 )
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 10 }
| gponVEIPServiceProfileName OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 11 }
| gponVEIPServiceAction OBJECT-TYPE
| SYNTAX INTEGER { active ( 1 ) , create ( 4 ) , destroy ( 6 ) , modify ( 7 ) }
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION "Column Description"
| ::= { gponVEIPServiceCfgEntry 12 }
| gponVEIPServiceIDCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GponVEIPServiceIDCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { gponOnuServiceConfig 4 }
| gponVEIPServiceIDCfgEntry OBJECT-TYPE
| SYNTAX GponVEIPServiceIDCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { portIndex }
| ::= { gponVEIPServiceIDCfgTable 1 }
| GponVEIPServiceIDCfgEntry ::= SEQUENCE {
| nextGponVEIPServiceID Integer32
| }
| nextGponVEIPServiceID OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { gponVEIPServiceIDCfgEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.50.1
| -- 1.3.6.1.4.1.5875.800.3.50.1
| gponServiceBandwidthCfg OBJECT IDENTIFIER ::= { gponConfig 1 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1
| -- 1.3.6.1.4.1.5875.800.3.50.1.1
| gponServiceBandwidthCfgTable OBJECT-TYPE
| SYNTAX SEQUENCE OF GponServiceBandwidthCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { gponServiceBandwidthCfg 1 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1
| gponServiceBandwidthCfgEntry OBJECT-TYPE
| SYNTAX GponServiceBandwidthCfgEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex, gponServiceType }
| ::= { gponServiceBandwidthCfgTable 1 }
| GponServiceBandwidthCfgEntry ::=
| SEQUENCE {
| gponServiceType
| Integer32,
| gponFixedBandwidth
| Integer32,
| gponAssureBandwidth
| Integer32,
| gponMaxBandwidth
| Integer32,
| gponBandwidthCfgAction
| RowStatus
| }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.1
| gponServiceType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Column Description:
| 1:IGMP
| 2:broadband Internet access
| 3:Voice
| 4:TDM
| 5:integrated service"
| ::= { gponServiceBandwidthCfgEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.2
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.2
| gponFixedBandwidth OBJECT-TYPE
| SYNTAX Integer32 (-2147483648..2147483647)
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { gponServiceBandwidthCfgEntry 2 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.3
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.3
| gponAssureBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { gponServiceBandwidthCfgEntry 3 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.4
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.4
| gponMaxBandwidth OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-write
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { gponServiceBandwidthCfgEntry 4 }
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.10
| -- 1.3.6.1.4.1.5875.800.3.50.1.1.1.10
| gponBandwidthCfgAction OBJECT-TYPE
| SYNTAX RowStatus
| MAX-ACCESS read-create
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { gponServiceBandwidthCfgEntry 10 }
| alarmStatus OBJECT IDENTIFIER
| ::= { oltData 60 }
| powerAlarmStatusTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PowerAlarmStatusEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { alarmStatus 1 }
| powerAlarmStatusEntry OBJECT-TYPE
| SYNTAX PowerAlarmStatusEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { powerIndex }
| ::= { powerAlarmStatusTable 1 }
| PowerAlarmStatusEntry ::= SEQUENCE {
| powerIndex Integer32,
| powerAlarmStatus INTEGER
| }
| powerIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { powerAlarmStatusEntry 1 }
| powerAlarmStatus OBJECT-TYPE
| SYNTAX INTEGER { normal ( 1 ) , lowVoltage ( 2 ) , fault ( 3 ) }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { powerAlarmStatusEntry 2 }
| fanAlarmStatusTable OBJECT-TYPE
| SYNTAX SEQUENCE OF FanAlarmStatusEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { alarmStatus 2 }
| fanAlarmStatusEntry OBJECT-TYPE
| SYNTAX FanAlarmStatusEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { slotIndex }
| ::= { fanAlarmStatusTable 1 }
| FanAlarmStatusEntry ::= SEQUENCE {
| fanAlarmStatus INTEGER
| }
| fanAlarmStatus OBJECT-TYPE
| SYNTAX INTEGER { normal ( 1 ) , stop ( 2 ) , abnormity ( 3 ) , nonChecking ( 4 ) }
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { fanAlarmStatusEntry 1 }
| currentAlarmTable OBJECT-TYPE
| SYNTAX SEQUENCE OF CurrentAlarmEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { alarmStatus 3 }
| currentAlarmEntry OBJECT-TYPE
| SYNTAX CurrentAlarmEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { currentAlarmIndex }
| ::= { currentAlarmTable 1 }
| CurrentAlarmEntry ::= SEQUENCE {
| currentAlarmIndex Integer32,
| currentAlarmCode Integer32,
| currentAlarmIfIndex Integer32,
| currentAlarmStatus Integer32,
| currentAlarmStatusFlag Integer32,
| currentAlarmBeginTime DateAndTime,
| currentAlarmEndTime DateAndTime,
| currentAlarmType Integer32,
| currentAlarmAdditionalText OCTET STRING
| }
| currentAlarmIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 1 }
| currentAlarmCode OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 2 }
| currentAlarmIfIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 3 }
| currentAlarmStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 4 }
| currentAlarmStatusFlag OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 5 }
| currentAlarmBeginTime OBJECT-TYPE
| SYNTAX DateAndTime
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 6 }
| currentAlarmEndTime OBJECT-TYPE
| SYNTAX DateAndTime
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 7 }
| currentAlarmType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 8 }
| currentAlarmAdditionalText OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { currentAlarmEntry 9 }
| hisAlarmTable OBJECT-TYPE
| SYNTAX SEQUENCE OF HisAlarmEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Description"
| ::= { alarmStatus 4 }
| hisAlarmEntry OBJECT-TYPE
| SYNTAX HisAlarmEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Row Description"
| INDEX { hisAlarmIndex }
| ::= { hisAlarmTable 1 }
| HisAlarmEntry ::= SEQUENCE {
| hisAlarmIndex Integer32,
| hisAlarmCode Integer32,
| hisAlarmIfIndex Integer32,
| hisAlarmStatus Integer32,
| hisAlarmStatusFlag Integer32,
| hisAlarmBeginTime DateAndTime,
| hisAlarmEndTime DateAndTime,
| hisAlarmType Integer32,
| hisAlarmAdditionalText OCTET STRING
| }
| hisAlarmIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 1 }
| hisAlarmCode OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 2 }
| hisAlarmIfIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 3 }
| hisAlarmStatus OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 4 }
| hisAlarmStatusFlag OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 5 }
| hisAlarmBeginTime OBJECT-TYPE
| SYNTAX DateAndTime
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 6 }
| hisAlarmEndTime OBJECT-TYPE
| SYNTAX DateAndTime
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 7 }
| hisAlarmType OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 8 }
| hisAlarmAdditionalText OBJECT-TYPE
| SYNTAX OCTET STRING
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION "Column Description"
| ::= { hisAlarmEntry 9 }
| -- 1.3.6.1.4.1.5875.800.3.101
| -- 1.3.6.1.4.1.5875.800.3.101
| objectIndex OBJECT IDENTIFIER ::= { oltData 101 }
| -- 1.3.6.1.4.1.5875.800.3.101.1
| -- 1.3.6.1.4.1.5875.800.3.101.1
| slotObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF SlotObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.1.1
| slotObjectIndexEntry OBJECT-TYPE
| SYNTAX SlotObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { slotIndex }
| ::= { slotObjectIndexTable 1 }
| SlotObjectIndexEntry ::=
| SEQUENCE {
| slotIndex
| Integer32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.1.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.1.1.1
| slotIndex OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { slotObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.2
| -- 1.3.6.1.4.1.5875.800.3.101.2
| onuObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF OnuObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 2 }
| -- 1.3.6.1.4.1.5875.800.3.101.2.1
| -- 1.3.6.1.4.1.5875.800.3.101.2.1
| onuObjectIndexEntry OBJECT-TYPE
| SYNTAX OnuObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { onuIndex }
| ::= { onuObjectIndexTable 1 }
| OnuObjectIndexEntry ::=
| SEQUENCE {
| onuIndex
| Unsigned32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.2.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.2.1.1
| onuIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { onuObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.3
| -- 1.3.6.1.4.1.5875.800.3.101.3
| uplinkObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF UplinkObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 3 }
| -- 1.3.6.1.4.1.5875.800.3.101.3.1
| -- 1.3.6.1.4.1.5875.800.3.101.3.1
| uplinkObjectIndexEntry OBJECT-TYPE
| SYNTAX UplinkObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { uplinkIndex }
| ::= { uplinkObjectIndexTable 1 }
| UplinkObjectIndexEntry ::=
| SEQUENCE {
| uplinkIndex
| Unsigned32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.3.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.3.1.1
| uplinkIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { uplinkObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.4
| -- 1.3.6.1.4.1.5875.800.3.101.4
| potsObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PotsObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 4 }
| -- 1.3.6.1.4.1.5875.800.3.101.4.1
| -- 1.3.6.1.4.1.5875.800.3.101.4.1
| potsObjectIndexEntry OBJECT-TYPE
| SYNTAX PotsObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { potsIndex }
| ::= { potsObjectIndexTable 1 }
| PotsObjectIndexEntry ::=
| SEQUENCE {
| potsIndex
| Unsigned32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.4.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.4.1.1
| potsIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { potsObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.5
| -- 1.3.6.1.4.1.5875.800.3.101.5
| portObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PortObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 5 }
| -- 1.3.6.1.4.1.5875.800.3.101.5.1
| -- 1.3.6.1.4.1.5875.800.3.101.5.1
| portObjectIndexEntry OBJECT-TYPE
| SYNTAX PortObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { portIndex }
| ::= { portObjectIndexTable 1 }
| PortObjectIndexEntry ::=
| SEQUENCE {
| portIndex
| Unsigned32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.5.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.5.1.1
| portIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { portObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.3.101.6
| -- 1.3.6.1.4.1.5875.800.3.101.6
| ponObjectIndexTable OBJECT-TYPE
| SYNTAX SEQUENCE OF PonObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Description"
| ::= { objectIndex 6 }
| -- 1.3.6.1.4.1.5875.800.3.101.6.1
| -- 1.3.6.1.4.1.5875.800.3.101.6.1
| ponObjectIndexEntry OBJECT-TYPE
| SYNTAX PonObjectIndexEntry
| MAX-ACCESS not-accessible
| STATUS current
| DESCRIPTION
| "Row Description"
| INDEX { ponIndex }
| ::= { ponObjectIndexTable 1 }
| PonObjectIndexEntry ::=
| SEQUENCE {
| ponIndex
| Unsigned32
| }
| -- 1.3.6.1.4.1.5875.800.3.101.6.1.1
| -- 1.3.6.1.4.1.5875.800.3.101.6.1.1
| ponIndex OBJECT-TYPE
| SYNTAX Unsigned32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Column Description"
| ::= { ponObjectIndexEntry 1 }
| -- 1.3.6.1.4.1.5875.800.1001
| -- 1.3.6.1.4.1.5875.800.1001
| equipTypeObjectId OBJECT IDENTIFIER ::= { standard 1001 }
| -- 1.3.6.1.4.1.5875.800.1001.1
| -- 1.3.6.1.4.1.5875.800.1001.1
| an5116v02 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 1 }
| -- 1.3.6.1.4.1.5875.800.1001.2
| -- 1.3.6.1.4.1.5875.800.1001.2
| an5116v06 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 2 }
| -- 1.3.6.1.4.1.5875.800.1001.11
| -- 1.3.6.1.4.1.5875.800.1001.11
| an5516v01 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 11 }
| -- 1.3.6.1.4.1.5875.800.1001.12
| -- 1.3.6.1.4.1.5875.800.1001.12
| an5516v04 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 12 }
| -- 1.3.6.1.4.1.5875.800.1001.14
| -- 1.3.6.1.4.1.5875.800.1001.14
| GT5116-06B OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 14 }
| -- 1.3.6.1.4.1.5875.800.1001.21
| -- 1.3.6.1.4.1.5875.800.1001.21
| an6016v01 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 21 }
| -- 1.3.6.1.4.1.5875.800.1001.101
| -- 1.3.6.1.4.1.5875.800.1001.101
| an2200v02 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 101 }
| -- 1.3.6.1.4.1.5875.800.1001.111
| -- 1.3.6.1.4.1.5875.800.1001.111
| an3300v02 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 111 }
| -- 1.3.6.1.4.1.5875.800.1001.112
| -- 1.3.6.1.4.1.5875.800.1001.112
| an3300v03 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 112 }
| -- 1.3.6.1.4.1.5875.800.1001.121
| -- 1.3.6.1.4.1.5875.800.1001.121
| an5006v15 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 121 }
| -- 1.3.6.1.4.1.5875.800.1001.122
| -- 1.3.6.1.4.1.5875.800.1001.122
| an5006v16 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 122 }
| -- 1.3.6.1.4.1.5875.800.1001.131
| -- 1.3.6.1.4.1.5875.800.1001.131
| an5006v20 OBJECT-TYPE
| SYNTAX Integer32
| MAX-ACCESS read-only
| STATUS current
| DESCRIPTION
| "Description"
| ::= { equipTypeObjectId 131 }
| END
| --
| -- GEPON-OLT-COMMON-MIB.my
| --

You can’t perform that action at this time.
You signed in with another tab or window. Reload to refresh your session. You signed out in another tab or window. Reload to refresh your session.